,Model##Other##,Nominal Tonnage##Other##,Fan Motor HP##Electrical_Power##Horsepower,Number of Fan Motors##Other##,Minimum Flow##Piping_Flow##us_gallons_per_minute,Maximum Flow##Piping_Flow##us_gallons_per_minute,Box Size##Other##,Unit Airflow##hvac_air_flow##cubic_feet_per_minute,Length##Length##Inches,Pan Width##Length##Inches,Lower Height##Length##Inches,Casing Width##Length##Inches,Casing Center Offset##Length##Inches,Casing Height##Length##Inches,Inlet Offset##Length##Inches,Inlet Elevation##Length##Inches,Number of Nozzles##Other##,PC1##Other##,PC2##Other##,E1##Other##,E2##Other##,Height##Length##Inches,Mounting Bolt Centerline##Length##Inches,Mounting Bolt Edge Distance##Length##Inches,Center Bolt Spacing##Length##Inches,Recommended Support Arrangement##Other##,Makeup Pipe Size##Pipe_Size##Inches,Drain Elevation##Length##Inches,Drain from Side##Length##Inches,Outlet Elevation##Length##Inches,Outlet from Blankoff##Length##Inches,Overflow Elevation##Length##Inches,Overflow from Blankoff##Length##Inches,Makeup Elevation##Length##Inches,Makeup from Blankoff##Length##Inches,Intake Setback##Length##Inches,Intake Base Elevation##Length##Inches,Fan Housing Radius##Length##Inches,Fan Housing Setback##Length##Inches,Fan Housing Width##Length##Inches,Fan Housing Elevation##Length##Inches,Fan Spacing##Length##Inches,Fan Configuration##Other##,Air Intake Clearance##Length##Feet,Operating Weight##Force##Pounds_Force,Minimum Inlet Size##Pipe_Size##Inches,Minimum Outlet Size##Pipe_Size##Inches,Number of Casings##Other##,Box Classification##Other##
VT1-N418-P,VT1-N418-P,418,40.0,2,794,2124,8x24,120600,139.75,94.375,80.75,93.25,0.5625,54.625,7.75,127.625,180,0.1045548,0.0202581,2,2,135.375,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,4.125,11,8.75,33.5,4.75,50,37.625,3,4,36,9,30,42,54,Series V 2 Fanwscrn : Configuration,9,18490,8,10,2,4
VT1-N440-O,VT1-N440-O,440,30.0,2,898,2092,8x24,106200,139.75,94.375,80.75,93.25,0.5625,77.375,9.5,148.625,180,0.1045548,0.0202581,2,2,158.125,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,4.125,11,8.75,33.5,4.75,50,37.625,3,4,36,9,30,42,54,Series V 2 Fanwscrn : Configuration,9,19110,8,10,2,4
VT1-N480-P,VT1-N480-P,480,40.0,2,1050,2274,8x24,115900,139.75,94.375,80.75,93.25,0.5625,77.375,9.5,148.625,180,0.1045548,0.0202581,2,2,158.125,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,4.125,11,8.75,33.5,4.75,50,37.625,3,4,36,9,30,42,54,Series V 2 Fanwscrn : Configuration,9,19490,8,10,2,4
VT1-N510-P,VT1-N510-P,510,40.0,2,1096,2322,8x24,111800,139.75,94.375,80.75,93.25,0.5625,94.125,9.5,165.375,180,0.1045548,0.0202581,2,2,174.875,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,4.125,11,8.75,33.5,4.75,50,37.625,3,4,36,9,30,42,54,Series V 2 Fanwscrn : Configuration,9,20890,8,10,2,4
