,Model##Other##,Nominal Tonnage##Other##,Fan Motor HP##Electrical_Power##Horsepower,Number of Fan Motors##Other##,Minimum Flow##Piping_Flow##us_gallons_per_minute,Maximum Flow##Piping_Flow##us_gallons_per_minute,Box Size##Other##,Unit Airflow##hvac_air_flow##cubic_feet_per_minute,Length##Length##Inches,Pan Width##Length##Inches,Lower Height##Length##Inches,Casing Width##Length##Inches,Casing Center Offset##Length##Inches,Casing Height##Length##Inches,Inlet Offset##Length##Inches,Inlet Elevation##Length##Inches,Number of Nozzles##Other##,PC1##Other##,PC2##Other##,Height##Length##Inches,Mounting Bolt Centerline##Length##Inches,Mounting Bolt Edge Distance##Length##Inches,Recommended Support Arrangement##Other##,Makeup Pipe Size##Pipe_Size##Inches,Drain Elevation##Length##Inches,Drain from Blankoff##Length##Inches,Outlet Elevation##Length##Inches,Outlet from Blankoff##Length##Inches,Overflow Elevation##Length##Inches,Overflow from Blankoff##Length##Inches,Makeup Elevation##Length##Inches,Makeup from Blankoff##Length##Inches,Intake Setback##Length##Inches,Intake Base Elevation##Length##Inches,Fan Housing Radius##Length##Inches,Fan Housing Setback##Length##Inches,Fan Housing Width##Length##Inches,Fan Housing Elevation##Length##Inches,Fan Spacing##Length##Inches,Fan Configuration##Other##,Air Intake Clearance##Length##Feet,Operating Weight##Force##Pounds_Force,Minimum Inlet Size##Pipe_Size##Inches,Minimum Outlet Size##Pipe_Size##Inches,Box Classification##Other##
VT0-132-L,VT0-132-L,132,15.0,1,273,619,4x12,30600,143.5,56.625,64.5,56.25,0.1875,76.625,11.25,129.875,52,0.086611195,0.00384082,141.125,137.5,1.1875,Series V Plan A-4 : Configuration,1,15.75,2.5,23.25,5.625,37,18.25,49.5,30.5,3,12,24,3,16,37,42,Series V 3 Fanwscrn : Configuration,5,5190,6,6,2
VT0-145-M,VT0-145-M,145,20.0,1,300,678,4x12,33670,143.5,56.625,64.5,56.25,0.1875,76.625,11.25,129.875,52,0.086611195,0.00384082,141.125,137.5,1.1875,Series V Plan A-4 : Configuration,1,15.75,2.5,23.25,5.625,37,18.25,49.5,30.5,3,12,24,3,16,37,42,Series V 3 Fanwscrn : Configuration,5,5200,6,6,2
VT0-155-N,VT0-155-N,155,25.0,1,321,723,4x12,36240,143.5,56.625,64.5,56.25,0.1875,76.625,11.25,129.875,52,0.086611195,0.00384082,141.125,137.5,1.1875,Series V Plan A-4 : Configuration,1,15.75,2.5,23.25,5.625,37,18.25,49.5,30.5,3,12,24,3,16,37,42,Series V 3 Fanwscrn : Configuration,5,5250,6,6,2
VT0-166-N,VT0-166-N,166,25.0,1,359,748,4x12,35265,143.5,56.625,64.5,56.25,0.1875,94.625,11.25,147.875,52,0.086611195,0.00384082,159.125,137.5,1.1875,Series V Plan A-4 : Configuration,1,15.75,2.5,23.25,5.625,37,18.25,49.5,30.5,3,12,24,3,16,37,42,Series V 3 Fanwscrn : Configuration,5,5650,6,6,2
VT0-176-O,VT0-176-O,176,30.0,1,382,792,4x12,37330,143.5,56.625,64.5,56.25,0.1875,94.625,11.25,147.875,52,0.086611195,0.00384082,159.125,137.5,1.1875,Series V Plan A-4 : Configuration,1,15.75,2.5,23.25,5.625,37,18.25,49.5,30.5,3,12,24,3,16,37,42,Series V 3 Fanwscrn : Configuration,5,5680,6,6,2
