,Model##Other##,Nominal Tonnage##Other##,Fan Motor HP##Electrical_Power##Horsepower,Number of Fan Motors##Other##,Minimum Flow##Piping_Flow##us_gallons_per_minute,Maximum Flow##Piping_Flow##us_gallons_per_minute,Box Size##Other##,Unit Airflow##hvac_air_flow##cubic_feet_per_minute,Length##Length##Inches,Pan Width##Length##Inches,Lower Height##Length##Inches,Casing Width##Length##Inches,Casing Center Offset##Length##Inches,Casing Height##Length##Inches,Inlet Offset##Length##Inches,Inlet Elevation##Length##Inches,Number of Nozzles##Other##,PC1##Other##,PC2##Other##,E1##Other##,E2##Other##,Height##Length##Inches,Mounting Bolt Centerline##Length##Inches,Mounting Bolt Edge Distance##Length##Inches,Center Bolt Spacing##Length##Inches,Recommended Support Arrangement##Other##,Makeup Pipe Size##Pipe_Size##Inches,Drain Elevation##Length##Inches,Drain from Blankoff##Length##Inches,Outlet Elevation##Length##Inches,Outlet from Blankoff##Length##Inches,Overflow Elevation##Length##Inches,Overflow from Blankoff##Length##Inches,Makeup Elevation##Length##Inches,Makeup from Blankoff##Length##Inches,Intake Setback##Length##Inches,Intake Base Elevation##Length##Inches,Fan Housing Radius##Length##Inches,Fan Housing Setback##Length##Inches,Fan Housing Width##Length##Inches,Fan Housing Elevation##Length##Inches,Fan Spacing##Length##Inches,Fan Configuration##Other##,Air Intake Clearance##Length##Feet,Operating Weight##Force##Pounds_Force,Minimum Inlet Size##Pipe_Size##Inches,Minimum Outlet Size##Pipe_Size##Inches,Box Classification##Other##
VT1-550-P,VT1-550-P,550,40.0,2,1029,2845,12x24,165060,139.75,142,100,140.75,0.625,54.625,7.75,146.875,300,0.1048635,0.010008898,2,2.28,154.625,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,3.375,12.5,27.125,29,4.75,40.5,65.25,3,4,48,20,24,54,42,Series V 3 Fanwscrn : Configuration,13.5,30590,8,12,4
VT1-680-O,VT1-680-O,680,40.0,2,1370,3286,12x24,163100,139.75,142,100,140.75,0.625,77.375,9.5,167.875,300,0.1048635,0.010008898,2,2.28,177.375,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,3.375,12.5,27.125,29,4.75,40.5,65.25,3,4,48,20,24,54,42,Series V 3 Fanwscrn : Configuration,13.5,32150,8,12,4
VT1-750-P,VT1-750-P,750,40.0,2,1588,3474,12x24,158600,139.75,142,100,140.75,0.625,94.125,9.5,184.625,300,0.1048635,0.010008898,2,2.28,194.125,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,3.375,12.5,27.125,29,4.75,40.5,65.25,3,4,48,20,24,54,42,Series V 3 Fanwscrn : Configuration,13.5,34090,8,12,4
VT1-800-Q,VT1-800-Q,800,50.0,2,1696,3700,12x24,170300,139.75,142,100,140.75,0.625,94.125,9.5,184.625,300,0.1048635,0.010008898,2,2.28,194.125,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,3.375,12.5,27.125,29,4.75,40.5,65.25,3,4,48,20,24,54,42,Series V 3 Fanwscrn : Configuration,13.5,34170,8,12,4
VT1-830-R,VT1-830-R,830,60.0,2,1762,3834,12x24,180500,139.75,142,100,140.75,0.625,94.125,9.5,184.625,300,0.1048635,0.010008898,2,2.28,194.125,127.5,1.375,17.25,Series V Plan A-8 2 Cell : Configuration,2,6.625,3.375,12.5,27.125,29,4.75,40.5,65.25,3,4,48,20,24,54,42,Series V 3 Fanwscrn : Configuration,13.5,34410,8,12,4
